**STEINEL Professional Presence detector**

**HF 360-2**

**KNX - Concealed wiring V3.2**

Type: Presence detector; Dimensions (L x W x H): 60 x 103 x 103 mm; Mains power supply: 30 V; Power supply, detail: KNX bus; Sensor Technology: High frequency; Application, place: Indoors; Installation site: ceiling; Installation: Concealed wiring; Mounting height: 2,50 – 4,00 m; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Reach, detail: 1 or 2 detection directions can be masked out by stickers for adjustment to the room situation.; HF-system: 5,8 GHz; Detection angle: 360 °; Angle of aperture: 140 °; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Detection: also through glass, wood and stud walls; Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Time setting: 10 sec – 1092 min; Constant-lighting control: Yes; Basic light level function: Yes; KNX functions: Comfort, Photo-cell controller, Individual pyro evaluation, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 4x, Humidity output, Presence output, Day / night function, Dewpoint, Temperature output, Logic gate; With bus coupling: Yes; Settings via: ETS software, Bluetooth, Bus; With remote control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; IP-rating: IP20; Material: Plastic; Ambient temperature: -25 – 50 °C; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; Version: KNX - Concealed wiring; PU1, EAN: 4007841064303

**Manufacturer** Steinel

**Prod. No.** 064303

**Ordering designation** HF 360-2 KNX - Concealed wiring

Deliver, install and set ready for operation